EXAMPLE

Create item budget for the realization of the inner bearing wall from brick blocks, width 240 mm. The wall has following proportions: width 5 000 mm, high 2 700 mm. In the wall is the opening for the door, width 900 mm, high 2 100 mm (own door is 800/1970 mm). Above the opening for the door there are 3 pieces of lintel (proportion in following table). Under the wall is spread the sealing sheet Bitagit, the width 1 000 mm, the length of the wall 5 000 mm. Under the sealing sheet there is realized the penetration coating (yield 0,0002 t/m2). Material reserve for bearing sheet is 15 %. The door is in the door case with the door step.  

N.	Number of Item	Name of Item	MU	Price/MU	Weight/MU	
1	311237133	Masonry from bricks HELUZ P 10 on MVC 5 width 24 cm	m2	956,00	0,22255	
2	317167211	Lintel Jistrop high, constructional 23,8/7/125 cm	kus	385,00	0,12919	
4	711111001	Isolation against dampness, water-soluble coating ALP	m2	7,20	0,00000	
5	766670011	Assembly of door case and wooden door	piece	1 160,00	0,00040	
6	766695212	Assembly of door steps, width up to 10 cm	piece	70,00	0,00001	
7	711141559	Isolation against dampness, sealing sheet 	m2	67,60	0,00041	
8	998766101	Moving with materials for joiner constructions, high up to 6 m	t	547,00	 	
9	998011001	Moving with materials for buildings from masonry, high up to 6 m	t	205,50	 	
10	998711101	Moving with materials for isolations against dampness, high up to 6 m	t	737,00	 	
11	11163110	Asphalt varnish for isolations ALP-PENETRAL ŽC, AC	t	22 514,00	1,00000	
12	61161755	Door inner 2/3 glass 80x197 veneer Mahagon	piece	3 405,60	0,02000	
13	61181272.A	Door case Sapeli w. 80 cm/w. of the wall 16-35cm	piece	3 354,00	0,03000	
14	62832134	Sealing sheet heavy Bitagit 40 mineral V 60 S 40	m2	67,93	0,00440	
15	61187396	Door step beech, length 8 cm, width 10 cm, high 2 cm	piece	66,98	0,00120	
SOLUTION

N.	Number of Item	Name of Item	MU	Amount	price/MU	Totally (CZK)	weight/MU	weight tot.(t)	
Part:	3	Vertical and complete constructions	 	 	 	 	 	 	

 		 	 	 	 	 	 	 	

 		 	 	 	 	 	 	 	

 	Totally for	3 Vertical and complete constructions	 	 	 	 	 	 	
Part:	99	Moving with materials on building site	 	 	 	 	 	 	

 		 	 	 	 	 	 	 	
 		 	 	 	 	 	 	 	
 	Totally for	99 Moving with materials on building site	 	 	 	 	 	 	
Part:	711	Isolation against water	 	 	 	 	 	 	

 		 	 	 	 	 	 	 	

 		 	 	 	 	 	 	 	

 		 	 	 	 	 	 	 	
 		 	 	 	 	 	 	 	
 	Totally for	711 Isolation against water	 	 	 	 	 	 	
Part:	766	Joiner constructions	 	 	 	 	 	 	

 		 	 	 	 	 	 	 	

									

 		 	 	 	 	 	 	 	
 	Totally for	766 Joiner constructions	 	 	 	 	 	 	
	 PRICE TOTALLY